(footprint "SW_PUSH_GT-TS201A-H0065"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "SMD Push button")
	(property "Reference" "REF**"
		(at 0 -1.9 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f37c6217-89ab-4ddc-bbe6-afbd3bda2c8f")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SW_PUSH_GT-TS201A-H0065"
		(at 0 1.9 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "101c4ded-80dc-452f-8836-1ea9b0a0416e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bbee9e6d-5e92-4659-acba-331007d6813e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ccb6c91b-8136-440c-8d66-75d1085b3352")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start -1.3 -0.2)
		(end -1.3 0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f2b7b6af-4ad1-4a83-84d9-53abbae04224")
	)
	(fp_line
		(start -0.9 -0.9)
		(end 0.9 -0.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d0ff0f57-fe6b-41fa-8c98-4f6c51a26876")
	)
	(fp_line
		(start -0.9 0.9)
		(end 0.9 0.9)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "996c7542-7ad8-43f2-998c-d92b119c23a2")
	)
	(fp_line
		(start 1.3 -0.2)
		(end 1.3 0.2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5d56e710-62be-4a1f-8fa7-e9d88e77d8a3")
	)
	(fp_circle
		(center 0 0)
		(end 0.4 0.3)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "Dwgs.User")
		(uuid "fa4fe3c5-a7f3-439e-9792-4591565f9f49")
	)
	(fp_rect
		(start -1.7 -1)
		(end 1.7 1)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "c66776b9-f544-484f-b128-b76d655cfe08")
	)
	(fp_text user "${REFERENCE}"
		(at 0 3.4 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "7a21f22d-724d-426c-b90f-5e52d071e8b8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.3 -0.6 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "3f0c5e83-28eb-4b64-9f4e-eddc481f3132")
	)
	(pad "1" smd roundrect
		(at 1.3 -0.6 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "8858e4f4-970e-4dd4-9a47-a75dbe5f83c8")
	)
	(pad "2" smd roundrect
		(at -1.3 0.6 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "62845d43-5606-4ffe-8de7-1341d72b9ccc")
	)
	(pad "2" smd roundrect
		(at 1.3 0.6 90)
		(size 0.6 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e0dc7117-c5c8-4f73-9045-0697d5eef612")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/footprints/Custom.pretty/SW_SMD_2.8x1.9mm.step"
		(offset
			(xyz 0 0 0.37)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
