(footprint "L_Changjiang_FTC201612S_Handsolder"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Inductor, Changjiang, FTC201612S, 2.0x1.6x1.2mm, (http://www.cjiang.com.cn/Pr_download_id_1117.html)")
	(tags "cjiang ftc molded power shielded")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
		(uuid "28557c84-fc02-430c-996f-31f3988e3335")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "L_Changjiang_FTC201612S_Handsolder"
		(at 0 1.8 0)
		(layer "F.Fab")
		(uuid "9e58d024-f1e4-470d-bf15-cd29cac2f99d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "45561fb5-50ee-4492-abe7-315f4d51be7e")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b720e81d-67cc-47ed-af06-a4ef207fb6b5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "KiLib_Generator" "inductor/SMD"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d83c2fd0-60af-497f-a6ee-a087e6a3a1b3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start -1.11 -1.11)
		(end 1.11 -1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "533f3b18-c036-49d9-94c1-ff1568b4e44c")
	)
	(fp_line
		(start 1.11 1.11)
		(end -1.11 1.11)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c833b2a5-107c-49f4-97d6-92126fe738d8")
	)
	(fp_rect
		(start -1.3 -1.1)
		(end 1.3 1.1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "d4ba70b1-22a0-4119-8298-610d2da734f2")
	)
	(fp_rect
		(start -1 -0.8)
		(end 1 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "5d45535d-d3c9-40f9-af9b-376c3512caa4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "9873e116-cc23-447a-8b7a-e03efa6cc548")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.725314 0.000657)
		(size 0.95 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "57afcdcd-9511-4dee-b753-97253e4e5f21")
	)
	(pad "2" smd roundrect
		(at 0.725 0)
		(size 0.95 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "38393e83-e1b7-4c63-a10d-9012fe6e6043")
	)
	(embedded_fonts no)
	(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Changjiang_FTC201612S.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
