
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MS561101BA03-50" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 10.922 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "MS561101BA03-50" (id 1) (at -10.16 -12.7 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "MS561101BA03-50:XDCR_MS561101BA03-50" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Comment" "MS561101BA03-50" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "TE Connectivity" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.1mm" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "SMD-8 Measurement Specialties" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/MS561101BA03-50/TE+Connectivity+Alcoswitch+Switches/view-part/?ref=eda" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "06/2017" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/MS561101BA03-50/TE+Connectivity+Alcoswitch+Switches/view-part/?ref=snap" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "MS561101BA03-50" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            BAROMETRIC PRESSURE SENSOR\n                        \n" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "TE Connectivity" (id 16) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "MS561101BA03-50_0_0"
      (rectangle (start -10.16 -10.16) (end 10.16 10.16)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 15.24 7.62 180.0) (length 5.08)
        (name "VDD"
          (effects (font (size 1.016 1.016)))
        )
        (number "1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 15.24 -7.62 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -15.24 -2.54 0) (length 5.08)
        (name "PS"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -15.24 2.54 0) (length 5.08)
        (name "~{CSB}"
          (effects (font (size 1.016 1.016)))
        )
        (number "4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input line (at -15.24 2.54 0) (length 5.08)
        (name "~{CSB}"
          (effects (font (size 1.016 1.016)))
        )
        (number "5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin output line (at 15.24 0.0 180.0) (length 5.08)
        (name "SDO"
          (effects (font (size 1.016 1.016)))
        )
        (number "6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 15.24 2.54 180.0) (length 5.08)
        (name "SDI/SDA"
          (effects (font (size 1.016 1.016)))
        )
        (number "7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin input clock (at 15.24 -2.54 180.0) (length 5.08)
        (name "SCLK"
          (effects (font (size 1.016 1.016)))
        )
        (number "8"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)