(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LM74610QDGKRQ1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
				(hide yes)
			)
		)
		(property "Value" "LM74610QDGKRQ1"
			(at -22.86 -16.51 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left top)
				(hide yes)
			)
		)
		(property "Footprint" "Regulators:SOP65P490X110-8N"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "MF" "Texas Instruments"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.10 mm"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Package" "VSSOP-8 Texas Instruments"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Price" "None"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/LM74610QDGKRQ1/Texas+Instruments/view-part/?ref=eda"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "STANDARD" "IPC-7351B"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "PARTREV" "B"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/LM74610QDGKRQ1/Texas+Instruments/view-part/?ref=snap"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MP" "LM74610QDGKRQ1"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Description_1" "0.48-V to 42-V, zero IQ automotive ideal diode controller"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify bottom)
				(hide yes)
			)
		)
		(symbol "LM74610QDGKRQ1_0_0"
			(rectangle
				(start -8.89 6.35)
				(end 11.43 -6.35)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(pin output line
				(at -13.97 3.81 0)
				(length 5.08)
				(name "VCAPH"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at -13.97 -1.27 0)
				(length 5.08)
				(name "ANODE"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin no_connect line
				(at -13.97 -3.81 0)
				(length 5.08)
				(name "NC_5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 16.51 3.81 180)
				(length 5.08)
				(name "VCAPL"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin output line
				(at 16.51 1.27 180)
				(length 5.08)
				(name "GATE_DRIVE"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin bidirectional line
				(at 16.51 -1.27 180)
				(length 5.08)
				(name "CATHODE"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin no_connect line
				(at 16.51 -3.81 180)
				(length 5.08)
				(name "NC_3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(symbol "LM74610QDGKRQ1_1_0"
			(pin bidirectional line
				(at -13.97 1.27 0)
				(length 5.08)
				(name "GATE_PD"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
