(footprint "SIQ-02FVS3_Rotary_Encoder"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -18.59 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "ba7b46b2-9682-4270-9a6b-4a12f1bb32e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "RotaryEncoder_Switch"
		(at 0.095 22.315 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "50753f76-5ae7-4065-94a5-b8fe2fcc1890")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79acd927-1b8f-4d26-b009-dbdc5c224f8a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "876880f6-e386-46ac-924d-cc14def4c0e9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start -5.3 0.5)
		(end -5.3 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "890a11e0-a0be-42e1-8701-0ef5c7ff9e23")
	)
	(fp_line
		(start -5.3 4.6)
		(end -5.3 2.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ec97f1a8-9b9f-4e9f-be3e-2b2a70471eb4")
	)
	(fp_line
		(start -5.3 7.3)
		(end -5.3 6.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d63e31ee-866a-49c2-a921-20a171bc8e10")
	)
	(fp_line
		(start -5.3 7.3)
		(end -4.8 7.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "686ee245-400a-4c05-bfa6-6cbc3c4e3dba")
	)
	(fp_line
		(start -4.199999 0)
		(end -5.3 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "06c0ac7a-e44c-4a3d-abf2-9e3773ceceb3")
	)
	(fp_line
		(start -3.2 7.3)
		(end -2.3 7.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "32938430-c96f-4639-993f-0b7931a35604")
	)
	(fp_line
		(start -0.7 7.3)
		(end 0.7 7.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "07b35564-37af-4583-8b62-8ca8e54e71d4")
	)
	(fp_line
		(start 0 -3.842113)
		(end -1.696517 -3.842113)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3d3bb76e-8a98-4042-bfa7-8052142addf9")
	)
	(fp_line
		(start 0 -3.842113)
		(end 1.696517 -3.842113)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "96d77e3a-e90d-4c69-94b6-1b0d5e71eeca")
	)
	(fp_line
		(start 2.2 7.3)
		(end 3.2 7.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9346d3a7-af32-4777-b38c-b88ec7528ab5")
	)
	(fp_line
		(start 4.8 7.3)
		(end 5.3 7.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0b84dfe3-08a0-4879-9ce8-6312777eb813")
	)
	(fp_line
		(start 5.3 0)
		(end 4.199999 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2a3c417b-afa5-4fd2-812c-b6c7fb29f6dd")
	)
	(fp_line
		(start 5.3 0.5)
		(end 5.3 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "8eff3935-1ec3-4390-bf38-5dcad2e35909")
	)
	(fp_line
		(start 5.3 4.6)
		(end 5.3 2.1)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "180fae24-c107-4ccd-a959-baf76fb6e0ce")
	)
	(fp_line
		(start 5.3 7.3)
		(end 5.3 6.2)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a4e5e6cb-1fea-4d83-8209-32354c71a4ed")
	)
	(fp_arc
		(start -4.16173 0)
		(mid -3.966729 -1.258991)
		(end -3.4 -2.4)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9a0726b9-a2b3-4645-b01b-3c6dbfabc9eb")
	)
	(fp_arc
		(start -2.6 -3.3)
		(mid -2.165597 -3.600027)
		(end -1.696996 -3.843204)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "baa13cb1-79be-408d-99ae-52d4594f6f39")
	)
	(fp_arc
		(start 1.696997 -3.843201)
		(mid 2.165598 -3.600026)
		(end 2.6 -3.3)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "06d2a8dd-12cb-4ccb-a4a5-e2058dbcfa66")
	)
	(fp_arc
		(start 3.383736 -2.488041)
		(mid 3.99072 -1.309259)
		(end 4.199999 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0a94b3a2-a3ac-42df-b112-7f8436d1ff3e")
	)
	(fp_circle
		(center 0 0)
		(end 0.2 -7.3)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "18ea68fa-3bde-4cb6-8c75-36fac3c2c6f7")
	)
	(fp_poly
		(pts
			(xy -5.4 7.5) (xy 5.4 7.5) (xy 5.4 -0.2) (xy 4.4 -0.2) (xy 4.1 -1.6) (xy 3.3 -2.9) (xy 1.7 -4.1)
			(xy -1.7 -4.1) (xy -3.4 -2.9) (xy -4.1 -1.6) (xy -4.4 -0.2) (xy -5.4 -0.2)
		)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "b8a1612c-4f69-47eb-ba61-6b42e492fb58")
	)
	(fp_circle
		(center 0 0)
		(end 7.25 0)
		(stroke
			(width 0.12)
			(type default)
		)
		(fill no)
		(layer "User.6")
		(uuid "8571485b-0b76-4965-b507-4cd0c1de0900")
	)
	(fp_text user "${REFERENCE}"
		(at 2.000001 -2.5 270)
		(layer "F.Fab")
		(uuid "cfcfabb7-c3df-4dd4-9398-fe3ec789f50f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole circle
		(at -3 4.5)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(uuid "dccc815a-cb9f-4e78-abe8-b005d71667e1")
	)
	(pad "" np_thru_hole circle
		(at 3 4.5)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(uuid "9f17f11a-a743-4fa9-ae80-f4b5cf926a85")
	)
	(pad "0" smd roundrect
		(at -5.4 1.3 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "386720b2-7740-40e0-8ed9-441addc6a90b")
	)
	(pad "0" smd roundrect
		(at -5.4 5.4 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "19006717-8dbc-4f3a-9578-94939be051e5")
	)
	(pad "0" smd roundrect
		(at -3.25269 -3.1 225)
		(size 0.85 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "a03f51b5-7272-4ccb-a9f8-e7702ebb9695")
	)
	(pad "0" smd roundrect
		(at 3.25266 -3.100001 315)
		(size 0.85 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "24304c68-9b3c-49dd-bf66-bcdf5b9bc1c7")
	)
	(pad "0" smd roundrect
		(at 5.4 1.3 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "aacf9c31-f6e2-4bd8-9d26-b5d0fb4c6895")
	)
	(pad "0" smd roundrect
		(at 5.4 5.4 90)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "1a01b36d-ed81-4407-b3d4-353bd328aff5")
	)
	(pad "1" smd roundrect
		(at -4 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "d5aa290b-1e90-4a87-8d16-d4009d799bf9")
	)
	(pad "2" smd roundrect
		(at -1.475 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "e92dc300-067b-4e48-98ac-3e2927a1145c")
	)
	(pad "3" smd roundrect
		(at 1.475 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "7a1eb37a-f926-427d-84ce-d875ad373ef1")
	)
	(pad "4" smd roundrect
		(at 4 7.7 180)
		(size 1.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
		(uuid "bb1570e4-9f75-4320-9f31-0f56ace8e9ab")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/footprints/Custom.pretty/SIQ-02FVS3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
